label 1 Filter Housing (2.75" x 5")
Text:
Stage 1 Sediment Filter
Select Series
1 micron
This filter reduces suspended solids such as Sand, Silt, Rust, Sediment and Particles from water
Operating Requirements:
Temp: Min 4°C 49°F, Max 52°C 125°F
Pressure: Min 35PSI 241KPA, Max 80PSI 551KPA
Manufacturers recommendation is to replace every 6-9 Months depending on incomming water quality
Warning- When intended use is for drinking water make sure water is microbiologically safe or adequate disinfection is performed before or after system.

label 2 Filter Housing (2.75" x 5")
Text:
Stage 2 Pre Carbon Filter
Select Series
This Filter absorbs organic contaminants such as chlorine, pesticides, herbicides and bad taste.
Operating Requirements:
Temp: Min 4°C 49°F, Max 52°C 125°F
Pressure: Min 35PSI 241KPA, Max 80PSI 551KPA
Manufacturers recommendation is to replace every 6-9 Months depending on incomming water quality
Warning- When intended use is for drinking water make sure water is microbiologically safe or adequate disinfection is performed before or after system.

label 3 Filter housing (2.75" x 5")
Text:
Stage 3 Carbon Filter
Select Series
5 Mircon
This filter absorbs the finer suspended organic contaminants such as chlorine, pesticides, herbicides, odors and bad tastes from many different compounds.
Operating Requirements:
Temp: Min 4°C 49°F, Max 52°C 125°F
Pressure: Min 35PSI 241KPA, Max 80PSI 551KPA
Manufacturers recommendation is to replace every 6-9 Months depending on incomming water quality
Warning- When intended use is for drinking water make sure water is microbiologically safe or adequate disinfection is performed before or after system.

Label 4 RO Membrane(3 3/8" x 2 1/8")
Text:
Stage 4 RO Membrane
Select Series
Removes chemicals such as metal ions, salts, chloride, chopper, lead, fluoride and many other harmful contaminants
Temp: Min 4°C 49°F, Max 52°C 125°F
Pressure: Min 35PSI 241KPA, Max 80PSI 551KPA
Manufacturers recommendation is to replace every 2-5 years depending on incomming water quality
Warning- When intended use is for drinking water make sure water is microbiologically safe or adequate disinfection is performed before or after system.

Label 5 Post Filter (4"x2.5")
Text:
Stage 5 Carbon Polishing Filter
Select Series
This filter polishes the purified water removing any left over bad taste or odor.
Maximum Flow: 0.5GPM
Maximum Pressure: 125 PSI
Maximum Temperature 100F
Life Expectancy: 1500Gallons
Warning- When intended use is for drinking water make sure water is microbiologically safe or adequate disinfection is performed before or after system.

label 6 Bracket (13.5"x 1  5/16")
Logo + Text "Select Series"
1(888) 621-0460