Finishes:

Exterior:
Roof, gutters, downpipes: 	Coloursteel – Sandstone Grey
Window joinery: 		Powdercoated – Sandstone Grey
Cedar weatherboard: 		Stained, Wood-X Avalanche
Plaster: 			Resene Half Cloud

Interior:
Flooring: 			Godfrey Hirst timber laminate flooring – Elegant oak
Carpet: 				Godfrey Hirst – Cockle 
Tiles: 				600x600, grey matte finish
Ceiling: 				Resene Alabaster
Trims, doors & windows: 	Resene Alabaster
Walls: 				Resene Sea Fog

Kitchen:
Benchtop: 			Granite stone, white polished
Joinery: 			Timberland, premium oak
Splashback:			Tiled, white, gloss
Appliances:			Fisher & Paykel stainless steel
Tapware:			Methven
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Specifications:

Construction:
Foundation:			Engineered concrete waffle slab over gravel raft
Framing:			90mm kiln dried SG8 framing
Intertenancy wall:		Gib Intertenancy Barrier system
Exterior wall insulation:		R2.6 glass wool batts
Ceiling insulation:		R4.0 glass wool batts
Midfloor insulation:		R2.2 glass wool batts
Intertenancy wall insulation	R2.2 glass wool batts

Exterior:
Roof:				Coloursteel tray profile
Fascia & gutter:			Coloursteel
Exterior Cladding:	Vertical cedar weatherboard and Rockcote Integra panel & plaster on ventilated cavity system
Window & door joinery:		Double glazed, powder coated aluminium
Front door:			Aluminium
Garage door:			Sectional door with automatic opener and remotes

Internal:
Ceiling height:			2.4m
Linings:				Painted gib, level 4 finish, aqualine to wet areas
Flooring:			Nylon died carpet with 11mm foam underlay
Internal doors:			Painted, flush finish, hollowcore
Door hardware:			Lever action handles, Satin Chrome
Wardrobe joinery:		Prefinished 16mm white melamine carcass
Landry joinery: 			Prefinished 16mm white melamine carcass and laminate benchtop

Bathroom:
Shower base & walls:		Tiled
Shower door:			Glazed
Vanity:				VCBC wall hung, in timberland oak
WC:				VCBC, back to wall
Tapware:			Methven, chrome
Heated towel rail:		Chrome
Wall heater:			Stainless steel
Mirror:				Wall hung mirror above vanity

Electrical:
Lighting	:			Recessed LED down lights
Heating:	Heat pump high wall mounted, Daikin or Mitsubishi, sized to meet Healthy Homes Regulations
Appliances:	Fisher & Paykel, induction hob, oven, rangehood & dishwasher
Water heater:			Electric 250L cylinder
Power:				Double outlets throughout
Smoke alarms:			To each floor

External works:
Driveway:			Concrete, exposed aggregate and sponge finish
Patio:				Concrete, sponge finish
Soft landscaping:		Plantings as per landscaping plan
Fencing:			To perimeter	
Other chattels:			Letterbox, washing line
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