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	NECESSARY INFORMATION FOR THE DESING(1)

	Product
	Body Hair Removal Cream 200ML

	Content
	200ML

	Name and function of the product
	EU: The function of the cosmetic product must be indicated in the design, unless it is clear from its presentation.

	Responsible person (name and address)
	EU: The name or registered name and the address of the responsible person. Such information may be abbreviated in so far as the abbreviation makes it possible to identify that person and his address. If several addresses are indicated, the one where the responsible person makes readily available the product information file shall be highlighted. The country of origin shall be specified for imported cosmetic products.

	Country of origin
	EU Regulation 1223/2009: Spain. The country of origin shall be specified for ONLY imported cosmetic products.

	Nominal content
[image: ]
	200ML e
Mínimum size: 3mm

	Internal code (mandatory for traceability) – it can be placed anywhere (visible or not visible) in the design
	Unit carton: Pending definition by CMW once the product will be confirmed
Tube: Pending definition by CMW once the product will be confirmed

	List of ingredients
	See document attached.
EU Market:

Ingredients: Aqua, Cetearyl Alcohol, Potassium Thioglycolate, Urea, Ceteareth-20, Glyceryl Stearate, Isopropyl Myristate, Calcium Hydroxide, Glycerin, Parfum, Sodium Hydroxide, Magnesium Aluminum Silicate, Sodium Gluconate, Dimethyl Phenethyl Acetate, Helianthus Annuus Seed Oil, Aloe Barbadensis Leaf Extract

EU: The list shall be preceded by the term ‘ingredients’ as it is indicated in the Cosmetic Regulation 1223/2009 for the different countries/languages.

*Attached you can find documents with info for USA & Canada market.
*Carton: Include as mandatory
*Tube: It is possible do not include it according to EU Reg. 1223/2009, art.19


	Marketing claims
	See document attached.

	General warnings
	See document attached.

	Mandatory warnings
	See document attached.


	Directions for use
	See document attached.


	Shelf life
[image: ]
	EU: 24 months
Include as follow:
[image: ]: See packaging

	PAO
[image: ]
	EU: 12M

	Hand-in-book symbol
[image: ]
	EU: Yes

	Mandatory symbols (OPRL, recycled logos for Spain, Conai logo…)
	Recycling logos

Only recycling and disposal labelling that is currently mandatory under the applicable national legislation in the EU Member States where the product is placed on the market should be included.
Until the harmonised packaging labelling requirements under the PPWR are officially adopted and become applicable, no PPWR-specific harmonised recycling/disposal symbols should be incorporated into the artwork.


	Optional symbols (FSC)
	N/A

	Batch code
	Carton: Leave a space of 28x8mm for the batch code/expiry date on the bottom.

	Barcode
	N/A



(1) The first design review will involve a complete check of the design, taking into consideration the requirements of Article 19 of the Cosmetics Regulation 1223/2009, during which COSMEWAX will propose useful modifications to the CUSTOMER, which will then be included in subsequent reviews. COSMEWAX will not be responsible for modifications which a customer makes to a design and that were not requested by Cosmewax, or when a customer does not give appropriate advance warning of modifications. In these cases, the CUSTOMER will be solely responsible. This revision does not ensure that translations into other languages other than English or Spanish are reliable.

	PACKAGING SPECIFICATIONS

	Component (2) 
	Quoted specifications
	Printing specifications

	Unit Carton 
Cutter guide code: Pending with final printer (Ulzama). Sent with other one which will be amend directly with final printer.
	Unit carton/GC1 or GC2 quality 270-330 g/m2/Dimensions: 63x52x180mmPrinted up to 6 colors/Matte or Gloss Acrylic Finish

	P04PR30 REV.00
· Text:
In all cases, please provide the fonts used with your files or 100% embedded in the PDF.
The texts in black must be embossed on GOLD and SILVER with a weight gain of 0.03mm.
Black texts must always be overprinted on Quad or Pantone color backgrounds.
We recommend the use of True Type fonts.
Positive impression: greater than 4 pts.
Negative impression: greater than 5 pts.
· Images:
Images must be in CMYK or CMYK + Pantones.
Maxi 8 Colors.
Composite files in EPS, TIFF or PDF.
Apply 40-30-30-100 CMYK -Support under Black Solid.
RGB files to CMYK.
JPEG OR LZW compressions should maintain high image quality.
Minimum recommended resolution 300 Dpi.
The addition of the superimposed color raster values must not exceed 320%. (ink rate).
Do not apply an ICC profile on the images.
· Nets:
The minimum size of the threads is 0.05 mm in positive, 0.10 mm in reserve and 0.10 mm colors
· Trapping:
White removal: 0.09mm backing (enriched black)
Coverage: 0.07 to 0.10mm
Trapping metallic inks: 0.03 mm

	Tube (Witoplast)
Cutter guide code: N/A
	PBL EVOH 200ML Tube (H: 157mm without cap, D:50mm), Orifice 7mm, up to 4 colours, Matte or Gloss Finish/Safety Seal Metal Free//White Gloss or Matt Screw on Cap


PBL tubes: flexo printing (CMYK or pantone). Texts only in pantone.


	Artworks in format Core IDRAW or illustrator
All fonts in curves
All fillings, gradients and outlines should be described in Pantone (CMYK only for flexo and silk screen)
Reading of barcodes can be assured only when color of bars is black on white background
The minimum size of one element is:
· Offset: 2,5 points (0,88mm) – In negative: 2,5 points (0,88mm)
· Silk screen: 2,5 points (0,88mm) – In negative: 3 points (1,06mm)
· Flexo: 2,5 points (0,88mm) – In negative: 2,5 points (0,88mm )
· Hot stamping: 5,5 points (1,92mm) – In negative 6 points (2,1mm)
The minimum thickness of printable line:
· Offset: 0,1 point (0,03mm) – In negative: 0,2 point (0,07mm)
· Silk screen: 0,2 points (0,07mm) – In negative: 0,2 points (0,07mm)
· Flexo: 0,1 point (0,03mm) – In negative: 0,2 point (0,07mm)
· Hot stamping: 0,5 points (0,17mm) – In negative: 0,75 points (0,26mm)
Registration between colors:
· Offset: ±0,1mm
· Silk screen: ±0,3mm
· Flexo: ±0,2mm
· Between hot stamping and other prints: ±0,35mm
· Between silk screen and offset: ±1mm
Screen density for silk screen and offset is 120 lpi
Objects in offset cannot be overprinted
Varnish (glossy or matt) layer is applying after offset and before silkscreen/hot-stamping prints
Photos used in artwork creation process have to be attached as a separated files in scale 1:1 in resolution minimum 300 dpi


(2) You will find the cutter guide in the Annex 4



	ANNEXES – ADDITIONAL INFORMATION


1. Quali-quantitative formulation
2. Marketing claims
3. Warnings & Directions for use
4. Cutter guides for the different components
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