**Concrete Pump Daily Check**

|  |  |  |  |
| --- | --- | --- | --- |
| NR | DESCRIPTION | YES/NO | COMMENTS |
| 1 | Check engine fluid levels (see engine manufacturer Maintenance schedule for additional requirements) |  |  |
| 2 | Check hydraulic tank fluid levels |  |  |
| 3 | Check flush box fluid levels |  |  |
| 4 | Check conditions of hydraulic oil for water or other contamination |  |  |
| 5 | Drain water from tank |  |  |
| 6 | Check hydraulics filter indicator condition |  |  |
| 7 | Lubricate lubrication points, during and after pumping |  |  |
| 8 | Inspect unit for fluid leaks, loose hoses, loose nuts, bolts, fasteners, etc |  |  |
|  | Additional notes: |  |  |
| 9 | Trailer Towing Safety Inspection   1. Brakes functional 2. Air pressure in tires is adequate and tire condition 3. All “lug nuts” are secure and in good condition |  |  |
| 10 | Additional notes: |  |  |

|  |  |
| --- | --- |
| Plant number |  |
| Hours |  |
| Time |  |
| Date |  |
| Print name |  |
| Sign name |  |