Author: jamesrwRD

The PowerAid on full charge can start the vehicle 15 times

1. Connect battery clamp of jumper cable to the vehicle battery termainal

2. Plug the cord of jumper cable into jump starter

3. start the vehicle

4. remove Jumper cable from jump start

5. Disconnect clamps from vehicle within seconds when vehicle starts

PowerAid on full charge can charge and iPhone 5 times, a notebook 2-3 hours—recharging the appliance to full power needs just 3 hours

Picture of unit only

LED jump start socket 19V 3.5A output indicator light switch USB 5V 2A output 12V2A output 12V 1A INPUT

Worlds smallest Jump Starter

Illumination

Flash Burst

The SOS

Jumper cables with clamps

Notebook cable & connector

Mobile phone
Cable & connector

For 12V vehicle products

The instruction LED illumination: press power button to turn on the light, press the power button again to change the mode.

Jumpstart . Recharge . Anytime. Anywhere

Poweraid2go.com

Parts List and Specifications

#	Parts Name	Qty
1	Main product	1
2	Switch cable A	1
3	Switch cable B	1
4	Mobile phone connector	8
5	Notebook connector	8
6	Home Adaptor	1
7	Car Adaptor	1
8	Jumper Cable with battery clamps	1

	Battery Power	1400aMh
	Operating Temp	00 – 600 C
	Battery Cell compositions	Li-Ion
	Item width	19 cm
	Item Height	6 cm
	Voltage	12 V
	Item length	28 cm
	Item Weight	1.2 kg
	Peak Current	400A

Thank
you

Recharge mobile phones

Pic of connectors

Recharge laptops

Thank
you

Pic of car adaptor

Pic of connectors

Website: Poweraid2go.com : email: info@poweraid2go.com