**The 699-418-X10 Long Range Handheld Transmitter**

The 699-418-X10 Handheld Transmitter is ideal for general-purpose remote control. It is suited for command applications that require longer distance transmission with up to ten functions capabilities. It has been pre-certified for FCC Part 15, reducing costs and time to market.

This remote control, available in 418 (standard), has a transmission range of up to 1000feet when combined with the [399-30 receiver](http://3abtechnologies.com/products/399-10.php). The transmitter unit can be configured with 1 to 10 buttons and the keypad and labeling can be modified to meet specific OEM customer requirements. Ease of use and security are dramatically enhanced by the on-board encoder, which allows instant creation of up to 16,777,216 (2^24) unique addresses. When paired with a [399-30 receiver](http://3abtechnologies.com/products/399-10.php), 699-418-X10 handheld transmitter identity can be determined and button permissions established. The unit uses a single 3V CR2032 lithium button cell.

**Features**

* 1 to 10 buttons.
* Heavy duty ABS enclosure.
* Customizable keypad.
* Developed for indoor and outdoor use.
* Membrane Life Expectancy: 1 million closures.

**Applications**

* General Remote Control.
* Keyless Entry.
* Garage / Gate Openers.
* Lighting Control.
* Call Systems.
* Home / Industrial Automation.
* Wire Elimination.