**The 399-30 provides features for both long and short range applications while providing reliable system control.**

The 10-position relay function module number 399-30 is a member of a 3AB product line. It is available in flange mount, compact plastic box. It is well suited for harsh environment and it can be easily integrated into variety of mobile and industrial applications.

**Features**

* Accepts input voltages (12 or 24 VDC)
* 10 Form C relay outputs
* Reverse bias protected
* Control up to 10 functions
* Factory programmed Latching and one Double Pole output
* Each output can source up to 10 Amps
* Rugged and reliable
* Long-life relays switch DC
* Compact in size
* Operational temperature – 40 to 85C
* Flange-mount box
* Frequency of operation – 418MHz

**Applications**

* General Control
* DC Motor and Solenoid Control
* Gate and Lighting Controller
* Hydraulic and Pneumatic Valve Driver